; @CESYSGEN IF BSP_NIC_AX88772
;IF BSP_NIC_AX88772
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\2965_30496\Default\Default\AX88772]
   	"DLL"="AX88772.DLL"
   	"Prefix"="ASX"
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\2965_30506\Default\Default\AX88772]
   	"DLL"="AX88772.DLL"
   	"Prefix"="ASX"

[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\AX88772]
   	"DLL"="AX88772.DLL"
   	"Prefix"="ASX"

[HKEY_LOCAL_MACHINE\Comm\AX88772]
   	"DisplayName"="ASIX AX88772 USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772.dll"
  
[HKEY_LOCAL_MACHINE\Comm\AX88772\Linkage]
   	"Route"=multi_sz:"AX887721","AX887722","AX887723","AX887724"

[HKEY_LOCAL_MACHINE\Comm\AX887721]
   	"DisplayName"="ASIX AX88772 USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX887721\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772 Driver Parameters:
;   "ConnectionType" ==> 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex"
; 		         	     8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
;   "FlowControl"   ==>  0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
;	"wakeup"		==>  0 = "Disable"; 2 = "Link-up"; 4 = "Magic Packet"; 8 = "Wakeup Frame"		
;						 6 = "Link-up" & "Magic Packet";
;						a = "Link-up" & "Wakeup Frame";
;						c = "Magic Packet" & "Wakeup Frame";
;						e = "All"
;						ps: "Wakeup Frame" is only for AX88772A chip
;===========================================================================
   	"ConnectionType"=dword:0
   	"FlowControl"=dword:3
	"WakeUp"=dword:0
;======================================================
;the follow only for AX88772A chip
;======================================================
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All";
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable";
	"VlanId"=dword:0				; 0 - 4095

[HKEY_LOCAL_MACHINE\Comm\AX887721\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?
		
[HKEY_LOCAL_MACHINE\Comm\AX887722]
   	"DisplayName"="ASIX AX88772 USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX887722\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772 Driver Parameters:
;   "ConnectionType" ==> 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex"
; 		         	     8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
;   "FlowControl"   ==>  0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
;	"wakeup"		==>  0 = "Disable"; 2 = "Link-up"; 4 = "Magic Packet"; 8 = "Wakeup Frame"		
;						 6 = "Link-up" & "Magic Packet";
;						a = "Link-up" & "Wakeup Frame";
;						c = "Magic Packet" & "Wakeup Frame";
;						e = "All"
;						ps: "Wakeup Frame" is only for AX88772A chip
;===========================================================================
   	"ConnectionType"=dword:0
   	"FlowControl"=dword:3
	"WakeUp"=dword:0
;======================================================
;the follow only for AX88772A chip
;======================================================
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All";
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable";
	"VlanId"=dword:0				; 0 - 4095

[HKEY_LOCAL_MACHINE\Comm\AX887722\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?

[HKEY_LOCAL_MACHINE\Comm\AX887723]
   	"DisplayName"="ASIX AX88772 USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX887723\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772 Driver Parameters:
;   "ConnectionType" ==> 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex"
; 		         	     8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
;   "FlowControl"   ==>  0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
;	"wakeup"		==>  0 = "Disable"; 2 = "Link-up"; 4 = "Magic Packet"; 8 = "Wakeup Frame"		
;						 6 = "Link-up" & "Magic Packet";
;						a = "Link-up" & "Wakeup Frame";
;						c = "Magic Packet" & "Wakeup Frame";
;						e = "All"
;						ps: "Wakeup Frame" is only for AX88772A chip
;===========================================================================
   	"ConnectionType"=dword:0
   	"FlowControl"=dword:3
	"WakeUp"=dword:0
;======================================================
;the follow only for AX88772A chip
;======================================================
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All";
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable";
	"VlanId"=dword:0				; 0 - 4095

[HKEY_LOCAL_MACHINE\Comm\AX887723\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?

[HKEY_LOCAL_MACHINE\Comm\AX887724]
   	"DisplayName"="ASIX AX88772 USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX887724\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772 Driver Parameters:
;   "ConnectionType" ==> 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex"
; 		         	     8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
;   "FlowControl"   ==>  0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
;	"wakeup"		==>  0 = "Disable"; 2 = "Link-up"; 4 = "Magic Packet"; 8 = "Wakeup Frame"		
;						 6 = "Link-up" & "Magic Packet";
;						a = "Link-up" & "Wakeup Frame";
;						c = "Magic Packet" & "Wakeup Frame";
;						e = "All"
;						ps: "Wakeup Frame" is only for AX88772A chip
;===========================================================================
   	"ConnectionType"=dword:0
   	"FlowControl"=dword:3
	"WakeUp"=dword:0
;======================================================
;the follow only for AX88772A chip
;======================================================
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All";
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable";
	"VlanId"=dword:0				; 0 - 4095

[HKEY_LOCAL_MACHINE\Comm\AX887724\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?
				
;ENDIF BSP_NIC_AX88772	
; @CESYSGEN ENDIF BSP_NIC_AX88772

